The function compares the number of pulses of the encoder that would cover that distance with the encoder’s values.

The distance between the IR Sensor and the first set of wheels is passed to the function

The actuator lifts the wheels

When they are same

IR Sensor detects the obstacle